

	That install applies to "Hardwired" (C) 1991 Crionics & Silents.


	That install requires WHDLoad and DIC to be in the path. Both
	can be found in the whdload package.


	You need 1 MB ChipMem and 0.5 MB OtherMem.
	You can quit the demo by pressing F10 (68010+ required).


	Sorrow that so a fine demo does run so bad on faster machines.
	Various things has been patched. Most parts are running now
	clear on my A2000/030/25. But there are problems on faster
	machines.
	Perhaps there will be better version later...


	full whdload package:	aminet:dev/misc/whdload#?.lha
	other installs:		http://www.whdload.org/


	This install is a coproduction of Mr Larmer & Wepl at the end of 1997.
	Enjoy the demo.

	version 1.1 (28.01.01) done by Harry:
	- transformation of pixelized vectors fixed for 50 mhz 68030

